**ITSS Embedded Linux – IT4946E**

**8.5 & 8.6**

8.5

1. Run the program1 and waiting for input enter.
2. Run program2. Confirm becoming the mutex unlock waiting of the program1.
3. Input Enter in the program1. Confirm program1 is unlocked.